
**QUECTEL EC25 KERNEL FLASHING PROCEDURE**

Step 1: Copy Paste the “QFlash\_V5.2\_EN” folder in your PC.


Step 2: Goto QFlash\_V5.2\_EN->Release

Step 3: Run “QFlash\_V5.2.exe”




QFlash\_V5.2.exe


Step 4 : In “QFlash\_V5.2.exe” click “Load FW Files” Button




Step 5 : After clicking “Load FW Files” Button. Goto the Kernel files folder in your PC.




Step 6 : Click “appsboot.mbn”




Step 7 : Click “Open”




Step 8 : Click “Configuration” and select “Sahara only”



Step 9 : Set your COM Port number and Baudrate



Step 10 : Click “Start”



Step 11: Kernel Uploading will start

